Text

Description automatically generated

SCC TECHNICAL INSPECTION FORM

EVENT \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_DATE DRIVER-\_\_\_\_\_\_\_\_\_\_\_

CAR MAKE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_MODEL \_\_\_\_\_\_\_\_\_\_\_\_\_ YEAR \_\_\_\_\_ CAR NUMBER \_\_\_

**INSTRUCTIONS (*Read carefully*):** Prior to bringing your car to the track or to the HPDE tech station, inspect each item on the car as listed. Consult a tech inspector if there are any questions. Have the top of the form filled out **prior** to going to the tech inspector. Making sure your car is track ready is ***your*** responsibility. More information and all rules are available online at [www.drivenasa.com.](http://www.drivenasa.com/)

# WHEELS & TIRES BRAKES

Tires in good condition pedal pressure

all lug nuts present & tight fluid level

lines (condition)

# STEERING & SUSPENSION

wheel bearings-front

wheel bearings-rear

steering play

# ENGINE

fluid leaks (oil, fuel, water)

radiator overflow tank

radiator hoses (condition)

battery secured (no bungees)

terminals covered

# Roll Cage

\_\_\_\_\_\_\_ Padding for contact areas

\_\_\_\_\_\_\_ Rear View Mirror

\_\_\_\_\_\_\_ Drivers Side Mirror

# SAFETY EQUIPMENT

\_\_\_\_\_\_\_ Harness in good condition and installed correctly, SFI dated within 4 years. Anti Sub Belt Recommended. 5 point!

helmet (Snell SA2010) or newer

\_\_\_\_\_\_\_ Eye Protection Required, Full Face or Goggles

\_\_\_\_\_\_\_\_Seat bolted in tight, frame mounted or attached to roll cage. No Floor mounted seats unless factory.

\_\_\_\_\_\_\_ Safety Cut off Switch located on dash or easy access by driver/ crew.

\_\_\_\_\_\_\_ Fire Extinguisher 2lb min with metal bracket, within Driver reach,

\_\_\_\_\_\_\_ Window net in good condition

\_\_\_\_\_\_\_ Fuel Cell securely mounted in good condition

\_\_\_\_\_\_\_ Fuel Cell Roll Over Flapper Valve

\_\_\_\_\_\_\_ Fuel Cell gas cap secure

\_\_\_\_\_\_\_ Driver Suit SAF 3.2/A1 or Higher Rating

\_\_\_\_\_\_\_ Driver Shoes SFI/FAI Rated or Leather with no holes

\_\_\_\_\_\_\_ Gloves SFI/FAI Rated

## I have inspected the above vehicle and take full responsibility for its condition on the track.

OWNER SIGNATURE: DATE

Inspector's comments (list any violations)

Inspectors stamp