**SELF TECH**

**INSPECTION FORM**

DRIVER: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ EVENT DATE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CAR MAKE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ MODEL: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ YEAR:\_\_\_\_\_\_\_\_\_\_\_

# INSTRUCTIONS

Prior to bringing your car to the track inspect each item on the car as listed, if you have any questions consult a professional. Remember - making sure your car is track ready is your responsibility.

# WHEELS & TIRES

Condition of tires (circle one)

NEW! GOOD WORN

\_\_\_\_\_ All lug nuts present & tight

\_\_\_\_\_ No hub caps

# STEERING & SUSPENSION

\_\_\_\_\_ Wheel bearings – front

\_\_\_\_\_ Wheel bearings – rear

\_\_\_\_\_ Steering play

# ENGINE

**\_\_\_\_\_** NOFluid leaks (oil, fuel, water)

\_\_\_\_\_ Radiator hose clamps secure

\_\_\_\_\_ Battery secured (proper bracket)

\_\_\_\_\_ Battery terminals covered

**HAVE READY AT TRACK:**

# BRAKES

\_\_\_\_\_ Good pedal pressure

\_\_\_\_\_ Brake fluid level

\_\_\_\_\_ Brake pad (good condition)

\_\_\_\_\_ Brake lights working

# SAFETY EQUIPMENT

\_\_\_\_\_ Approved roll bars in open cars – See owner’s manual

\_\_\_\_\_ Seat belts or harness in working order

\_\_\_\_\_ Helmet (Snell SA2015 rating or newer)

\_\_\_\_\_ Covered battery inside cockpit

# MISCELLANEOUS

\_\_\_\_\_ Gas cap secured

\_\_\_\_\_ No wires exposed

\_\_\_\_\_ Seats bolted tight

* No loose objects in car or trunk. Remove spare tire, jack, floor mats, dash mats, paper, etc. These items can be removed at the track before your session starts.
* A tech/session sticker placed on top LEFT (driver side) of the windshield, once you have checked-in

Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_