

**Technical Inspection and Equipment Checklist** **2021**

Driver Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Car Year, Make, and Model\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Register Car Number \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Body Suspension**

[ ] Functional brake lights [ ] Wheel bearings properly adjusted, no play

[ ] Hood, doors, trunk and body panels secured [ ] No excessive suspension deflection

[ ] Windshield has no major cracks. [ ] Brake system bled, adjusted and level

 Windows must be way all the way up or all the down. between Min and Max

[ ] Gas cap intact and tightened [ ] No excessive steering play

[ ] Numbers clearly affixed on both sides of vehicle

**Interior** [ ] No frayed or leaking hydraulic brake,

[ ] Seats well secured steering, or, clutch lines

[ ] Seat belts required in good working order and condition [ ] 50 % or greater remaining brake [ ] All loose items (including floor mats) removed from lining/pad required

 cockpit, glove box, console, trunk, etc. [ ] Shock absorbers in good working order

[ ] Pedals have free return and in good operating condition

 Firm brake pedal **Engine and Drivetrain Driver Equipment**

[ ] No fluid leaks of any kind (gas, oil or coolant) [ ] M/SA/K Snell 2005 or later. DOT only not [ ] Battery properly secured (NO Bungees) allowed

[ ] All hoses, oil, fuel, and water,with no visible signs [ ] Goggles/face shields (eye protection) for

 of damage. Securely clamped/tightened open cars

[ ] Exhaust system securely attached [ ] Proper footwear, no sandals or opened

[ ] Throttle return is safe and positive toe shoes

[ ] Radiator secure, proper overflow container

**Wheels and Tires** **Exhaust**

[ ] Tires properly inflated and defect free [ ] 98 db rule strictly enforced. One chance for [ ] Street tires 2/32” average tread depth, no cord repair/modification. If it fails, vehicle will not

 visible. Competition tires (slicks) allowed be allowed to run any more. [ ] All lug nuts/knockoffs torqued to spec,

 hubcaps, trim rings, center caps, removed

[ ] No visible cracks in wheels

**CERTIFICATION**

I hereby certify that I have personally performed the inspections and completed the above Technical Inspection and Equipment Checklist. I have found, or corrected, each item to be in compliance with applicable standards.I further certify that I have read and understand all rules and regulations relating to this event and agree to abide with. I understand that completion of these checklists is a minimum requirement of the event, but in no way assures the safety of my vehicle and that the preparation of my vehicle is the responsibility of myself and/or the driver/owner. I further understand that the ruling of the NWAA Event Chair, in regards to participation in this event, will be final.

Driver’s Name(Printed) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Driver’s Signature (Signed)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

NWWA Staff Signature (Signed)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_