****

**PDX TECH SHEET**

**Complete this sheet before coming to the track and bring it with you.**

Driver: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Run Group: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Car #: \_\_\_\_\_\_

Car Make:\_\_\_\_\_\_\_\_\_\_\_\_\_ Model:\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Color:\_\_\_\_\_\_\_\_\_\_\_\_\_ Year: \_\_\_\_

*The entrant/participant is responsible for the safety of his/her vehicle. Neither the tech inspectors, the event organizers, nor the sanctioning body will be held responsible for the safety of this vehicle. Have a qualified mechanic check over your car and make certain everything is in good working order for an event such as this. Event tech inspectors will inspect those items listed as required. Please have all the items listed above as required items out prior to entering the inspection line, along with this form.*

**DRIVER SAFETY**

\_\_\_\_ Helmet (Snell M/SA 2000 or newer, SFI, FIA)

\_\_\_\_ Shoes must be solid and in reasonable condition

\_\_\_\_ Seatbelts/Harness must be in good condition

\_\_\_\_ A Proper ROLLBARwhen it is required

\_\_\_\_ Rollbar padding

\_\_\_\_ Seats bolted securely

\_\_\_\_ Interior & trunk clear of loose items

**BRAKES**

\_\_\_\_ Pads are less than half worn

\_\_\_\_ Fluid is clear. Reservoir is full. Dot 4 recommended.

\_\_\_\_ Pedal is firm

\_\_\_\_ All Brake lights are working

\_\_\_\_ Master Cylinder/Calipers are not leaking

\_\_\_\_ Rotors have no cracks or discoloration

**TIRES & WHEELS**

\_\_\_\_ Adequate tire tread, speed rating, good condition

\_\_\_\_ All lug nuts present & torqued

\_\_\_\_ Hubcaps removed

\_\_\_\_ Wheels - No cracks or structural damage

**SUSPENSION & STEERING**

\_\_\_\_ Wheel bearings - no play

\_\_\_\_ Ball joints in good condition

\_\_\_\_ No excessive steering play.

\_\_\_\_ Shocks - no leaking

**ENGINE & DRIVE TRAIN**

\_\_\_\_ Check all fluid levels, belts, and hoses. Tighten all caps

\_\_\_\_ No fluid leaks (oil, fuel, water)

\_\_\_\_ Battery secured (no bungees)

\_\_\_\_ Battery terminals covered

\_\_\_\_ Overflow containers present

\_\_\_\_ Exhaust system functional (may have to meet sound restrictions)

\_\_\_\_ Throttle has quick, positive return

\_\_\_\_ Fuel cap tightened

**OTHER**

\_\_\_\_ Windshield has no large cracks

\_\_\_\_ Windshield wipers function properly

\_\_\_\_ Outside & Rear View mirrors

\_\_\_\_ Car numbers visible on both sides of car

Signed:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Driver or Mechanic